A picture containing metal, tripod


Description automatically generatedThe Product

* New platform with “saloon”-type automatic closing door.
* Work platform designed for all work up to 3.44 m height.
* Ideal for finishing work such as carpentry, dry lining and general maintenance
* Safe, enclosed working with generous 410x436mm platform area
* Lightweight – No fatigue when transporting/moving around site
* A picture containing handcart

  Description automatically generated2-year warranty.

Specification

* Deep tool pocket
* Stabilisers legs with millimetric adjustment (4 Tread models and up)
* 10 cm height toe boards
* Heavy duty platform lock hook when in use
* 150 mm tilt wheels for easy transportation
* Max folded width 700mm and folded depth 300mm
* EN131-7 – 150KG weight loading



|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | A | B | C | D | E | F |  |
| Code | Description | Platform Height m | Working Height m | Base Width m | Base Projection m | Closed Depth m | Closed Length  m | Weight  (KG) |
| GMAXP2 | 2 Tread Gmax + | 0.48 | 2.48 | 0.70 | 0.89 | 0.3 | 1.82 | 12.8 |
| GMAXP3 | 3 Tread Gmax + | 0.72 | 2.72 | 0.70 | 1.04 | 0.3 | 2.08 | 13.5 |
| GMAXP4 | 4 Tread Gmax + | 0.96 | 2.96 | 0.70 / 1.43 | 1.19 | 0.3 | 2.33 | 15.5 |
| GMAXP5 | 5 Tread Gmax + | 1.20 | 3.20 | 0.70 / 1.43 | 1.35 | 0.3 | 2.58 | 18.5 |
| GMAXP6 | 6 Tread Gmax + | 1.44 | 3.44 | 0.70 / 1.43 | 1.50 | 0.3 | 2.85 | 19.0 |