The Product

* New platform with “halo”-type automatic closing overhead barrier
* Work platform designed for all work up to 3.68 m height.
* Ideal for finishing work such as carpentry, dry lining and general maintenance
* Safe, enclosed working with generous 410x436mm platform area
* Lightweight – No fatigue when transporting/moving around site
* 2-year warranty.

Specification

* Deep tool pocket
* Stabilisers legs with millimetric adjustment (4 Tread models and up)
* 10 cm height toe boards
* Heavy duty platform lock hook when in use
* 150 mm tilt wheels for easy transportation
* Max folded width 700mm and folded depth 360mm
* EN131-7 – 150KG weight loading



|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | A | B | C | D | E | F |  |
| Code | Description | Platform Height m | Working Height m | Base Width m | Base Projection m | Closed Depth m | Closed Lengthm | Weight(KG) |
| GMAX2 | 2 Tread Gmax  | 0.48 | 2.48 | 0.70 | 0.98 | 0.36 | 1.74 | 12.0 |
| GMAX3 | 3 Tread Gmax | 0.72 | 2.72 | 0.70 | 1.16 | 0.36 | 2.00 | 13.0 |
| GMAX4 | 4 Tread Gmax | 0.96 | 2.96 | 0.70 /1.43 | 1.34 | 0.36 | 2.28 | 15.5 |
| GMAX5 | 5 Tread Gmax | 1.20 | 3.20 | 0.70 / 1.43 | 1.52 | 0.36 | 2.54 | 18.0 |
| GMAX6 | 6 Tread Gmax | 1.44 | 3.44 | 0.70 / 1.43 | 1.70 | 0.366 | 2.82 | 19.0 |
| GMAX7 | 7 Tread Gmax | 1.68 | 3.68 | 0.70 / 1.43 | 1.88 | 0.36 | 3.10 | 20.0 |