The Product

* Introducing the aluminium swingback / builders step from Murdoch International
* Tested to 50,000 cycles to withstand the most vigorous usage
* From 4 Tread – 12 Tread
* Two aluminium locking arms for security
* Steel fittings/hinges for strength and rigidity
* 10 year warranty

Specification

* Large 85mm anti-slip treads
* Large 82mm front profile for easy climbing
* Two aluminium locking arms
* Large, anti-slip, all round moulded feet
* 150KG load rated
* EN131 Professional

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Code | Description | Open Depth mA | Open Height m B | Base Width mC | Closed Length mD | Max Working Height mV | WeightKG |
| SHR804 | 4 Tread Aluminium Builders / Swingback Stepladder  | 0.69 | 0.86 | 0.43 | 0.99 | 2.11 | 3.9 |
| SHR805 | 5 Tread Aluminium Builders / Swingback Stepladder | 0.85 | 1.06 | 0.45 | 1.22 | 2.31 | 5.0 |
| SHR806 | 6 Tread Aluminium Builders / Swingback Stepladder | 0.99 | 1.27 | 0.48 | 1.45 | 2.52 | 5.5 |
| SHR808 | 8 Tread Aluminium Builders / Swingback Stepladder | 1.31 | 1.69 | 0.54 | 1.91 | 2.94 | 7.3 |
| SHR810 | 10 Tread Aluminium Builders / Swingback Stepladder | 1.62 | 2.11 | 0.59 | 2.37 | 3.36 | 9.5 |
|  SHR812 | 12 Tread Aluminium Builders / Swingback Stepladder | 1.92 | 2.53 | 0.64 | 2.83 | 3.78 | 12.0 |

