The Product

* Introducing the Issima platform step by Murdoch international
* A close-up of a tower

  Description automatically generated with low confidenceTested to 50,000 cycles to withstand the most vigorous usage
* From 3 Tread – 12 Tread
* 275 x 260mm platform area for safe footing made out of composite material of nylon and fibreglass for ultimate strength
* 10 year warranty
* Made in Italy

Specification

* Large 80mm anti-slip treads
* Diagram

  Description automatically generatedTreads connected like rungs for massive strength
* Simple to use platform lock
* Large 70x20mm box section stiles
* Two anti-splay straps
* Large, anti-slip, all round moulded feet
* 150KG load rated
* EN131 Professional
* Comes with user friendly bucket hook and tool tray
* Handrails available as an accessory

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Code | Description | Open Height m  A | Platform Height m  B | Closed Length m  C | Base Width m  D | Max Working Height m  H | Weight  KG |
| A07IS150 | 3 Tread Issima Platform Step | 1.28 | 0.66 | 1.36 | 0.44 | 2.66 | 5.0 |
| A07IS175 | 4 Tread Issima Platform Step | 1.51 | 0.89 | 1.61 | 0.46 | 2.89 | 5.9 |
| A07IS200 | 5 Tread Issima Platform Step | 1.74 | 1.12 | 1.86 | 0.49 | 3.12 | 6.8 |
| A07IS225 | 6 Tread Issima Platform Step | 1.97 | 1.35 | 2.11 | 0.51 | 3.35 | 7.7 |
| A07IS275 | 8 Tread Issima Platform Step | 2.43 | 1.81 | 2.61 | 0.56 | 3.81 | 9.5 |
| A07IS325 | 10 Tread Issima Platform Step | 2.89 | 2.27 | 3.11 | 0.61 | 4.27 | 12.5 |
| A07IS375 | 12 Tread Issima Platform Step | 3.35 | 2.73 | 3.61 | 0.66 | 4.73 | 14.9 |
| A50CORR67 | Single Handrail for Issima Step |  |  | 0.8 |  |  | 1.2 |