A ladder leaning against a wall

Description automatically generated with medium confidenceThe Product

* Introducing the new Dmax extension ladder from Murdoch International
* Deployable stabiliser bar makes transportation and storage easier than traditional ladders with fixed stabiliser bar
* Comfortable working with a deep 39mm D shaped rung
* Strong ridged profile design helps to prevent dents to stiles
* 10 year warranty

A white ladder leaning against a wall

Description automatically generated with low confidence

Specification

* Deep 39mm D shaped rung
* 1200mm deployable stabiliser bar
* 300mm rung spacing
* Heavy duty, manual rung lock
* Max folded width 700mm and folded depth 300mm
* EN131 Professional

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Code | Description | Closed Length m | Extended Length m | Base Width mm (closed/  open) | Stile Dims mm | Weight  KG |
| **Double Extension** |  |  |  |  |  |  |
| A10059082255 | 2 x 8 Dmax Double Extension Ladder | 2.55 | 4.06 | 780/1200 | 58/25 | 11.0 |
| A10069102315 | 2 x 10 Dmax Double Extension Ladder | 3.15 | 5.26 | 780/1200 | 68/25 | 15.0 |
| A10069112345 | 2 x 11 Dmax Double Extension Ladder | 3.45 | 5.86 | 780/1200 | 68/25 | 16.0 |
| A10069132405 | 2 x 13 Dmax Double Extension Ladder | 4.15 | 6.36 | 780/1200 | 68/25 | 20.0 |
| A10100152465 | 2 x 15 Dmax Double Extension Ladder | 4.65 | 8.76 | 780/1200 | 100/25 | 26.0 |
| **Triple Extension** |  |  |  |  |  |  |
| A10069083255 | 3 x 8 Dmax Triple Extension Ladder | 2.55 | 5.56 | 780/1200 | 58/25 | 18.0 |
| A10069103315 | 3 x 10 Dmax Triple Extension Ladder | 3.15 | 7.36 | 780/1200 | 68/25 | 21.5 |
| A10084113345 | 3 x 11 Dmax Triple Extension Ladder | 3.45 | 8.26 | 780/1200 | 85/25 | 24.0 |
| A10100133405 | 3 x 13 Dmax Triple Extension Ladder | 4.15 | 10.06 | 780/1200 | 100/25 | 30.0 |